Main :

* Write screen (r28, r29, r30)
* Lecture mémoire (r25, r26, r27)

Timer 0 interrupt :

* Bouton (r20, r21)
* Son (r24)
* Volume (r23)
* User led

UART interrupt (r16, r17)

Lettre r22, r23(I)

R18,r19, , r20(I+cp), r31

Init r20

Adc, io, main OK

Uart r16, r17, r18

Screen r19-r22

Spi r23-r25